{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["设备","材料"],"read":"whole","date_system":"1900"}

{"sheet":"设备","index":0,"n_rows":19,"n_cols":6,"rows_kept":19}
["南食堂三楼设备清单"]
["序号","型号","数量","单价","合计","备注"]
[1,"GMV-NDR140PMS/A",17,null,null,"带回风箱、含遥控"]
[2,"GMV-NDR80PMS/A",6,null,null,"带回风箱、含遥控"]
[3,"GMV-NDR71PS/B",4,null,null,"带回风箱、含遥控"]
[4,"GMV-NR125T/D",4]
[5,"GMV-NR36T/D",3]
[6,"GMV-NR50T/D",2]
[7,"GMV-400WM/A1",1,null,null,"利旧"]
[8,"GMV-1010WM/A2",3]
[9,"KFR-120TW",1,null,null,"利旧"]
[10,"KFR-12OLW",1,null,null,"利旧"]
[11,"KFR-35GW",4,null,null,"利旧"]
[12,"KFR-50GW",1,null,null,"利旧"]
[13,"KFR-72LW",2]
[14,"KFR-72LW",1,null,null,"利旧"]
[15,"FGR7.2/D2",5,null,null,"含线控"]
[16,"FGR10/D2",3,null,null,"含线控"]
[17,"格力遥控器",15]

{"sheet":"材料","index":1,"n_rows":34,"n_cols":7,"rows_kept":34}
["南食堂材料清单"]
["序号","材料名称","单位","数量","单价","合计","备注"]
[1,"镀锌铁皮风管（厚度1MM)","平方",653,null,null,"单价含吊装、保温附件（保温B1级）"]
[2,"散流器（铝合金）","只",69,null,null,"600*600"]
[3,"出风口（铝合金）","只",2,null,null,"250*250"]
[4,"出风口（铝合金）","只",8,null,null,"200*1100"]
[5,"回风口（铝合金）","只",31,null,null,"200*1200（带滤网）"]
[6,"长条出风口（铝合金）","条",4,null,null,"200*6100"]
[7,"长条回风口（铝合金）","条",2,null,null,"200*6100（带滤网）"]
[8,"散流器帆布软接","只",69]
[9,"空调回风软接","只",35,null,null,"回风箱至回风口"]
[10,"出风软接","只",35,null,null,"出风口至风管"]
[11,"VRV内机安装","台",36]
[12,"VRV外机机吊装","项",1]
[13,"VRV内机安装材料（均价）","台",36]
[14,"VRV外机安装（均价）","套",2,null,null,"外机放置3楼顶就近设备基础，橡胶减震"]
[15,"药水（F410A)","KG"]
[16,"打孔","项",1]
[17,"冷凝水管","项",1]
[18,"KFR-120TW安装","套",1,null,null,"利旧铜管由管道井至3楼屋面"]
[19,"KFR-12OLW安装","套",1,null,null,"利旧，外机挂外墙"]
[20,"KFR-35GW安装","套",4,null,null,"利旧，外机由外墙至屋面"]
[21,"KFR-50GW安装","套",1,null,null,"利旧，外机由外墙至屋面"]
[22,"KFR-72LW安装","套",2,null,null,"新购。外机挂外墙"]
[23,"KFR-72LW安装","套",1,null,null,"利旧外机挂外墙"]
[24,"FGR7.2/D2安装（含材料）","套",4,null,null,"铜管由管道井至屋面，挖机支架挂女儿墙"]
[25,"FGR10/D2安装（含材料）","套",3,null,null,"铜管由外墙至2楼顶，外机挂外墙"]
[26,"FGR7.2/D2安装（含材料）","套",1,null,null,"铜管由外墙至3楼顶，外机挂外墙"]
["总计"]
[]
["注："]
[1,"所有空调冷凝水管排至2楼平台，不得与大楼雨水管、排污管相接。"]
[2,"铜管国内品牌挤压管、保温厚度不低于15MM，B1级防火"]
[3,"铜管、水管外侧保温接口胶水粘连并黑色包扎带包扎、 "]